'  '  '          '  '/'

INSTRUMENT          {

NIMROD          Instrument name
/home/aks45/Gudrun/GudrunN/run/NIMROD/Cycle18_4/Marinakis/          Gudrun input file directory:
/home/aks45/Gudrun/GudrunN/RawData/NIMROD/cycle18_4/          Data file directory
raw          Data file type
StartupFiles/NIMROD/NIMROD84modules+9monitors+LAB5Oct2012Detector.dat          Detector calibration file name
4          User table column number for phi values
NIMROD84modules+9monitors5Oct2012Groups.dat          Groups file name
StartupFiles/NIMROD/NIMRODdeadtimeNone.cor          Deadtime constants file name
4 5          Spectrum number(s) for incident beam monitor
0  0          Wavelength range [Å] for monitor normalisation
8 9          Spectrum number(s) for transmission monitor
0.0001          Incident monitor quiet count constant
0.0001          Transmission monitor quiet count constant
0  0          Channel numbers for spike analysis
5          Spike analysis acceptance factor
0.05  12  0.1          Wavelength range to use [Å] and step size
200            No. of smooths on monitor
0.1  50.0  0.05          Min, Max and step in x-scale (-ve for logarithmic binning)
0  0  0  0          0 0 0 0 to end input of specified values
1          Groups acceptance factor 
4          Merge power
0          Subtract single atom scattering?
2          By channel?
20.0          Incident flight path [m]
0          Spectrum number to output diagnostic files
StartupFiles/NIMROD/sears91_gudrun.dat          Neutron scattering parameters file
1          Scale selection: 1 = Q, 2 = d-space, 3 = wavelength, 4 = energy, 5 = TOF
1          Subtract wavelength-binned data?
/home/aks45/Gudrun/Gudrun2014/Gudrun          Folder where Gudrun started
/home/aks45/Gudrun/Gudrun2014/Gudrun/StartupFiles/SLS          Folder containing the startup file
0.03          Logarithmic step size
1          Hard group edges?
12          Number of iterations
0          Tweak the tweak factor(s)?

}

BEAM          {

FLATPLATE          Sample geometry
2          Number of beam profile values
1.0  1.0            Beam profile values (Maximum of 50 allowed currently)
0.05  0.2  100          Step size for absorption and m.s. calculation and no. of slices
10          Angular step for corrections [deg.]          
-1.5  1.5  -1.5  1.5          Incident beam edges relative to centre of sample [cm]
-2.0  2.0  -2.1  2.1          Scattered beam edges relative to centre of sample [cm]
StartupFiles/NIMROD/spectrum000.dat          Filename containing incident beam spectrum parameters
1.0          Overall background factor 
0.0          Sample dependent background factor
0.0          Shielding attenuation coefficient [per m per A] 

}

NORMALISATION          {

3  1          Number of  files and period number
NIMROD00064139.raw          NORMALISATION data files
NIMROD00064140.raw          NORMALISATION data files
NIMROD00064141.raw          NORMALISATION data files
1  1          Number of  files and period number
NIMROD00064138.raw          NORMALISATION BACKGROUND data files
1          Force calculation of corrections?
V  0  0.9485          Normalisation atomic composition
Nb  0  0.0515          Normalisation atomic composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.15  0.15          Upstream and downstream thicknesses [cm]
0.0  5          Angle of rotation and sample width (cm)
-0.072          Density atoms/Å^3?
200          Temperature for normalisation Placzek correction
TABLES          Total cross section source
*          Normalisation differential cross section filename
0.01          Lower limit on smoothed normalisation  
1.05          Normalisation degree of smoothing
0.0          Minimum normalisation signal to background ratio

}

SAMPLE BACKGROUND          {

2  1          Number of  files and period number
NIMROD00064142.raw          SAMPLE BACKGROUND data files
NIMROD00064143.raw          SAMPLE BACKGROUND data files

}

SAMPLE Empty TiZr Container          {

5  1          Number of  files and period number
NIMROD00064146.raw          SAMPLE Empty TiZr Container data files
NIMROD00064147.raw          SAMPLE Empty TiZr Container data files
NIMROD00064148.raw          SAMPLE Empty TiZr Container data files
NIMROD00064149.raw          SAMPLE Empty TiZr Container data files
NIMROD00064150.raw          SAMPLE Empty TiZr Container data files
1          Force calculation of sample corrections?
Ti  0  7.16          Composition
Zr  0  3.438          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.107  0.107          Upstream and downstream thicknesses [cm]
0  5          Angle of rotation and sample width (cm)
-0.0542          Density atoms/Å^3?
0          Temperature for Placzek correction:
TRANSMISSION          Total cross section source
1.0          Tweak factor
0          Top hat width (1/Å) for cleaning up Fourier Transform
0.0          Minimum radius for FT  [Å]
0.1          g(r) broadening at r = 1A [A]
0  0          0   0          to finish specifying wavelength range of resonance
0.0  1.0  0          Exponential amplitude and decay [1/A]
*  0  0          * 0 0 to specify end of exponential parameter input
1.0          Normalisation correction factor
NIMROD00064146.msubw01          Name of file containing self scattering as a function of wavelength [A]
0          Normalise to:Nothing
20.0          Maximum radius for FT [A]
0          Output units: b/atom/sr
0.2          Power for broadening function e.g. 0.5
0.03          Step size [A] 
0          Analyse this sample? 
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

GO          

SAMPLE NO at 120K, 1.3 bar          {

4  1          Number of  files and period number
NIMROD00064162.raw          SAMPLE NO at 120K, 1.3 bar data files
NIMROD00064163.raw          SAMPLE NO at 120K, 1.3 bar data files
NIMROD00064164.raw          SAMPLE NO at 120K, 1.3 bar data files
NIMROD00064165.raw          SAMPLE NO at 120K, 1.3 bar data files
1          Force calculation of sample corrections?
N  0  1.0          Composition
O  0  1.0          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.0893  0.0893          Upstream and downstream thicknesses [cm]
0  10          Angle of rotation and sample width (cm)
1.268          Density Units:  gm/cm^3?
0          Temperature for Placzek correction:
TRANSMISSION          Total cross section source
1.0          Tweak factor
-10          Top hat width (1/Å) for cleaning up Fourier Transform
0.9          Minimum radius for FT  [Å]
0.05          g(r) broadening at r = 1A [A]
0  0          0   0          to finish specifying wavelength range of resonance
0.0  1.0  0          Exponential amplitude and decay [1/A]
*  0  0          * 0 0 to specify end of exponential parameter input
1.0          Normalisation correction factor
NIMROD00064162.msubw01          Name of file containing self scattering as a function of wavelength [A]
0          Normalise to:Nothing
20.0          Maximum radius for FT [A]
0          Output units: b/atom/sr
0.05          Power for broadening function e.g. 0.5
0.03          Step size [A] 
1          Analyse this sample? 
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

CONTAINER 2mm TiZr flat plate cell          {

5  1          Number of  files and period number
NIMROD00064146.raw          CONTAINER 2mm TiZr flat plate cell data files
NIMROD00064147.raw          CONTAINER 2mm TiZr flat plate cell data files
NIMROD00064148.raw          CONTAINER 2mm TiZr flat plate cell data files
NIMROD00064149.raw          CONTAINER 2mm TiZr flat plate cell data files
NIMROD00064150.raw          CONTAINER 2mm TiZr flat plate cell data files
Ti  0  7.16          Composition
Zr  0  3.438          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.1  0.1          Upstream and downstream thicknesses [cm]
0  10          Angle of rotation and sample width (cm)
-0.0542          Density atoms/Å^3?
TRANSMISSION          Total cross section source
1.12          Tweak factor
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

GO          

SAMPLE NO at 127K, 2 bar          {

10  1          Number of  files and period number
NIMROD00064167.raw          SAMPLE NO at 127K, 2 bar data files
NIMROD00064168.raw          SAMPLE NO at 127K, 2 bar data files
NIMROD00064169.raw          SAMPLE NO at 127K, 2 bar data files
NIMROD00064170.raw          SAMPLE NO at 127K, 2 bar data files
NIMROD00064171.raw          SAMPLE NO at 127K, 2 bar data files
NIMROD00064172.raw          SAMPLE NO at 127K, 2 bar data files
NIMROD00064173.raw          SAMPLE NO at 127K, 2 bar data files
NIMROD00064174.raw          SAMPLE NO at 127K, 2 bar data files
NIMROD00064175.raw          SAMPLE NO at 127K, 2 bar data files
NIMROD00064176.raw          SAMPLE NO at 127K, 2 bar data files
1          Force calculation of sample corrections?
N  0  1.0          Composition
O  0  1.0          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.0893  0.0893          Upstream and downstream thicknesses [cm]
0  10          Angle of rotation and sample width (cm)
1.236          Density Units:  gm/cm^3?
0          Temperature for Placzek correction:
TRANSMISSION          Total cross section source
1.0          Tweak factor
-10          Top hat width (1/Å) for cleaning up Fourier Transform
0.9          Minimum radius for FT  [Å]
0.05          g(r) broadening at r = 1A [A]
0  0          0   0          to finish specifying wavelength range of resonance
0.0  1.0  0          Exponential amplitude and decay [1/A]
*  0  0          * 0 0 to specify end of exponential parameter input
1.0          Normalisation correction factor
NIMROD00064167.msubw01          Name of file containing self scattering as a function of wavelength [A]
0          Normalise to:Nothing
20.0          Maximum radius for FT [A]
0          Output units: b/atom/sr
0.05          Power for broadening function e.g. 0.5
0.03          Step size [A] 
1          Analyse this sample? 
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

CONTAINER 2mm TiZr flat plate cell          {

5  1          Number of  files and period number
NIMROD00064146.raw          CONTAINER 2mm TiZr flat plate cell data files
NIMROD00064147.raw          CONTAINER 2mm TiZr flat plate cell data files
NIMROD00064148.raw          CONTAINER 2mm TiZr flat plate cell data files
NIMROD00064149.raw          CONTAINER 2mm TiZr flat plate cell data files
NIMROD00064150.raw          CONTAINER 2mm TiZr flat plate cell data files
Ti  0  7.16          Composition
Zr  0  3.438          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.1  0.1          Upstream and downstream thicknesses [cm]
0  10          Angle of rotation and sample width (cm)
-0.0542          Density atoms/Å^3?
TRANSMISSION          Total cross section source
1.12          Tweak factor
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

GO          

SAMPLE NO at 134K, 4 bar          {

2  1          Number of  files and period number
NIMROD00064178.raw          SAMPLE NO at 134K, 4 bar data files
NIMROD00064179.raw          SAMPLE NO at 134K, 4 bar data files
1          Force calculation of sample corrections?
N  0  1.0          Composition
O  0  1.0          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.0893  0.0893          Upstream and downstream thicknesses [cm]
0  10          Angle of rotation and sample width (cm)
1.194          Density Units:  gm/cm^3?
0          Temperature for Placzek correction:
TRANSMISSION          Total cross section source
1.0          Tweak factor
-10          Top hat width (1/Å) for cleaning up Fourier Transform
0.9          Minimum radius for FT  [Å]
0.05          g(r) broadening at r = 1A [A]
0  0          0   0          to finish specifying wavelength range of resonance
0.0  1.0  0          Exponential amplitude and decay [1/A]
*  0  0          * 0 0 to specify end of exponential parameter input
1.0          Normalisation correction factor
NIMROD00064178.msubw01          Name of file containing self scattering as a function of wavelength [A]
0          Normalise to:Nothing
20.0          Maximum radius for FT [A]
0          Output units: b/atom/sr
0.05          Power for broadening function e.g. 0.5
0.03          Step size [A] 
1          Analyse this sample? 
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

CONTAINER 2mm TiZr flat plate cell          {

5  1          Number of  files and period number
NIMROD00064146.raw          CONTAINER 2mm TiZr flat plate cell data files
NIMROD00064147.raw          CONTAINER 2mm TiZr flat plate cell data files
NIMROD00064148.raw          CONTAINER 2mm TiZr flat plate cell data files
NIMROD00064149.raw          CONTAINER 2mm TiZr flat plate cell data files
NIMROD00064150.raw          CONTAINER 2mm TiZr flat plate cell data files
Ti  0  7.16          Composition
Zr  0  3.438          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.1  0.1          Upstream and downstream thicknesses [cm]
0  10          Angle of rotation and sample width (cm)
-0.0542          Density atoms/Å^3?
TRANSMISSION          Total cross section source
1.12          Tweak factor
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

GO          

SAMPLE NO at 144K, 9 bar          {

2  1          Number of  files and period number
NIMROD00064181.raw          SAMPLE NO at 144K, 9 bar data files
NIMROD00064182.raw          SAMPLE NO at 144K, 9 bar data files
1          Force calculation of sample corrections?
N  0  1.0          Composition
O  0  1.0          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.0893  0.0893          Upstream and downstream thicknesses [cm]
0  10          Angle of rotation and sample width (cm)
1.129          Density Units:  gm/cm^3?
0          Temperature for Placzek correction:
TRANSMISSION          Total cross section source
1.0          Tweak factor
-10          Top hat width (1/Å) for cleaning up Fourier Transform
0.9          Minimum radius for FT  [Å]
0.05          g(r) broadening at r = 1A [A]
0  0          0   0          to finish specifying wavelength range of resonance
0.0  1.0  0          Exponential amplitude and decay [1/A]
*  0  0          * 0 0 to specify end of exponential parameter input
1.0          Normalisation correction factor
NIMROD00064181.msubw01          Name of file containing self scattering as a function of wavelength [A]
0          Normalise to:Nothing
20.0          Maximum radius for FT [A]
0          Output units: b/atom/sr
0.05          Power for broadening function e.g. 0.5
0.03          Step size [A] 
1          Analyse this sample? 
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

CONTAINER 2mm TiZr flat plate cell          {

5  1          Number of  files and period number
NIMROD00064146.raw          CONTAINER 2mm TiZr flat plate cell data files
NIMROD00064147.raw          CONTAINER 2mm TiZr flat plate cell data files
NIMROD00064148.raw          CONTAINER 2mm TiZr flat plate cell data files
NIMROD00064149.raw          CONTAINER 2mm TiZr flat plate cell data files
NIMROD00064150.raw          CONTAINER 2mm TiZr flat plate cell data files
Ti  0  7.16          Composition
Zr  0  3.438          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.1  0.1          Upstream and downstream thicknesses [cm]
0  10          Angle of rotation and sample width (cm)
-0.0542          Density atoms/Å^3?
TRANSMISSION          Total cross section source
1.12          Tweak factor
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

GO          

SAMPLE NO at 99K          {

9  1          Number of  files and period number
NIMROD00064192.raw          SAMPLE NO at 99K data files
NIMROD00064193.raw          SAMPLE NO at 99K data files
NIMROD00064194.raw          SAMPLE NO at 99K data files
NIMROD00064195.raw          SAMPLE NO at 99K data files
NIMROD00064196.raw          SAMPLE NO at 99K data files
NIMROD00064197.raw          SAMPLE NO at 99K data files
NIMROD00064198.raw          SAMPLE NO at 99K data files
NIMROD00064199.raw          SAMPLE NO at 99K data files
NIMROD00064200.raw          SAMPLE NO at 99K data files
1          Force calculation of sample corrections?
N  0  1.0          Composition
O  0  1.0          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.0893  0.0893          Upstream and downstream thicknesses [cm]
0  10          Angle of rotation and sample width (cm)
1.3          Density Units:  gm/cm^3?
0          Temperature for Placzek correction:
TRANSMISSION          Total cross section source
1.0          Tweak factor
-          Top hat width (1/Å) for cleaning up Fourier Transform
0.9          Minimum radius for FT  [Å]
0.05          g(r) broadening at r = 1A [A]
0  0          0   0          to finish specifying wavelength range of resonance
0.0  1.0  0          Exponential amplitude and decay [1/A]
*  0  0          * 0 0 to specify end of exponential parameter input
1.0          Normalisation correction factor
NIMROD00064192.msubw01          Name of file containing self scattering as a function of wavelength [A]
0          Normalise to:Nothing
20.0          Maximum radius for FT [A]
0          Output units: b/atom/sr
0.05          Power for broadening function e.g. 0.5
0.03          Step size [A] 
0          Analyse this sample? 
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

CONTAINER 2mm TiZr flat plate cell          {

5  1          Number of  files and period number
NIMROD00064146.raw          CONTAINER 2mm TiZr flat plate cell data files
NIMROD00064147.raw          CONTAINER 2mm TiZr flat plate cell data files
NIMROD00064148.raw          CONTAINER 2mm TiZr flat plate cell data files
NIMROD00064149.raw          CONTAINER 2mm TiZr flat plate cell data files
NIMROD00064150.raw          CONTAINER 2mm TiZr flat plate cell data files
Ti  0  7.16          Composition
Zr  0  3.438          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.1  0.1          Upstream and downstream thicknesses [cm]
0  10          Angle of rotation and sample width (cm)
-0.0542          Density atoms/Å^3?
TRANSMISSION          Total cross section source
1.12          Tweak factor
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

GO          


END          
1
Date and time last written:  20210908 12:38:54          
N