'  '  '          '  '/'

INSTRUMENT          {

NIMROD          Instrument name
/home/aks45/Gudrun/GudrunN/run/NIMROD/MCM41GasAbsorption/          Gudrun input file directory:
/home/aks45/Gudrun/GudrunN/RawData/NIMROD/RB1800005/          Data file directory
nxs          Data file type
StartupFiles/NIMROD/NIMROD84modules+9monitors+LAB5Oct2012Detector.calib          Detector calibration file name
4          User table column number for phi values
StartupFiles/NIMROD/NIMROD84modules+9monitors+LAB5Oct2012Groups.dat          Groups file name
StartupFiles/NIMROD/NIMRODdeadtimeNone.cor          Deadtime constants file name
4 5          Spectrum number(s) for incident beam monitor
0  0          Wavelength range [Å] for monitor normalisation
8 9          Spectrum number(s) for transmission monitor
0.0001          Incident monitor quiet count constant
0.0001          Transmission monitor quiet count constant
0  0          Channel numbers for spike analysis
5          Spike analysis acceptance factor
0.05  12  0.1          Wavelength range to use [Å] and step size
200            No. of smooths on monitor
0.02  50.0  -0.05          Min, Max and step in x-scale (-ve for logarithmic binning)
0  0  0  0          0 0 0 0 to end input of specified values
1          Groups acceptance factor 
4          Merge power
0          Subtract single atom scattering?
2          By channel?
20.0          Incident flight path [m]
0          Spectrum number to output diagnostic files
StartupFiles/NIMROD/sears91_gudrun.dat          Neutron scattering parameters file
1          Scale selection: 1 = Q, 2 = d-space, 3 = wavelength, 4 = energy, 5 = TOF
1          Subtract wavelength-binned data?
/home/aks45/Gudrun/Gudrun2014/Gudrun          Folder where Gudrun started
/home/aks45/Gudrun/Gudrun2014/Gudrun/StartupFiles/SLS          Folder containing the startup file
0.03          Logarithmic step size
1          Hard group edges?
StartupFiles/NIMROD/NIMROD84modules+9monitors+LAB.nexus_txt          NeXus definition file
4          Number of iterations
0          Tweak the tweak factor(s)?

}

BEAM          {

FLATPLATE          Sample geometry
2          Number of beam profile values
1.0  1.0            Beam profile values (Maximum of 50 allowed currently)
0.05  0.2  100          Step size for absorption and m.s. calculation and no. of slices
10          Angular step for corrections [deg.]          
-1.5  1.5  -1.5  1.5          Incident beam edges relative to centre of sample [cm]
-2.0  2.0  -2.1  2.1          Scattered beam edges relative to centre of sample [cm]
StartupFiles/NIMROD/spectrum000.dat          Filename containing incident beam spectrum parameters
1.0          Overall background factor 
0.0          Sample dependent background factor
0.0          Shielding attenuation coefficient [per m per A] 

}

NORMALISATION          {

1  1          Number of  files and period number
NIMROD00053768.nxs          NORMALISATION data files
1  1          Number of  files and period number
NIMROD00053769.nxs          NORMALISATION BACKGROUND data files
1          Force calculation of corrections?
V  0  0.9485          Normalisation atomic composition
Nb  0  0.0515          Normalisation atomic composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.15  0.15          Upstream and downstream thicknesses [cm]
0.0  5          Angle of rotation and sample width (cm)
-0.072          Density atoms/Å^3?
200          Temperature for normalisation Placzek correction
TABLES          Total cross section source
*          Normalisation differential cross section filename
0.01          Lower limit on smoothed normalisation  
1.05          Normalisation degree of smoothing
0.0          Minimum normalisation signal to background ratio

}

SAMPLE BACKGROUND          {

1  1          Number of  files and period number
NIMROD00053326.nxs          SAMPLE BACKGROUND data files

}

SAMPLE Empty TiZr Container          {

1  1          Number of  files and period number
NIMROD00053329.nxs          SAMPLE Empty TiZr Container data files
1          Force calculation of sample corrections?
Ti  0  7.16          Composition
Zr  0  3.438          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.107  0.107          Upstream and downstream thicknesses [cm]
0  5          Angle of rotation and sample width (cm)
-0.0542          Density atoms/Å^3?
0          Temperature for Placzek correction:
TRANSMISSION          Total cross section source
1.0          Tweak factor
0          Top hat width (1/Å) for cleaning up Fourier Transform
0.0          Minimum radius for FT  [Å]
0.1          g(r) broadening at r = 1A [A]
0  0          0   0          to finish specifying wavelength range of resonance
0.0  1.0  0          Exponential amplitude and decay [1/A]
*  0  0          * 0 0 to specify end of exponential parameter input
1.0          Normalisation correction factor
NIMROD00053329.msubw01          Name of file containing self scattering as a function of wavelength [A]
0          Normalise to:Nothing
20.0          Maximum radius for FT [A]
0          Output units: b/atom/sr
0.2          Power for broadening function e.g. 0.5
0.03          Step size [A] 
0          Analyse this sample? 
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

GO          

SAMPLE  Dry MCM41 at 88K Adjust tweak factor 1 ver 2          {

4  1          Number of  files and period number
NIMROD00053339.nxs          SAMPLE  Dry MCM41 at 88K Adjust tweak factor 1 ver 2 data files
NIMROD00053340.nxs          SAMPLE  Dry MCM41 at 88K Adjust tweak factor 1 ver 2 data files
NIMROD00053341.nxs          SAMPLE  Dry MCM41 at 88K Adjust tweak factor 1 ver 2 data files
NIMROD00053342.nxs          SAMPLE  Dry MCM41 at 88K Adjust tweak factor 1 ver 2 data files
1          Force calculation of sample corrections?
Si  0  1.0          Composition
O  0  2.11          Composition
H  0  0.22          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.1  0.1          Upstream and downstream thicknesses [cm]
0  10          Angle of rotation and sample width (cm)
-0.02484          Density atoms/Å^3?
0          Temperature for Placzek correction:
TRANSMISSION          Total cross section source
5.45          Tweak factor
-10.0          Top hat width (1/Å) for cleaning up Fourier Transform
0.7          Minimum radius for FT  [Å]
0.05          g(r) broadening at r = 1A [A]
0  0          0   0          to finish specifying wavelength range of resonance
0.0  1.0  0          Exponential amplitude and decay [1/A]
*  0  0          * 0 0 to specify end of exponential parameter input
1.0          Normalisation correction factor
*          Name of file containing self scattering as a function of wavelength [A]
0          Normalise to:Nothing
20.0          Maximum radius for FT [A]
0          Output units: b/atom/sr
0.05          Power for broadening function e.g. 0.5
0.03          Step size [A] 
0          Analyse this sample? 
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

CONTAINER 2mm TiZr flat plate cell          {

1  1          Number of  files and period number
NIMROD00053329.nxs          CONTAINER 2mm TiZr flat plate cell data files
Ti  0  7.16          Composition
Zr  0  3.438          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.1  0.1          Upstream and downstream thicknesses [cm]
0  10          Angle of rotation and sample width (cm)
-0.0542          Density atoms/Å^3?
TRANSMISSION          Total cross section source
1.0          Tweak factor
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

GO          

SAMPLE  N2 in MCM41 at 88K          {

9  1          Number of  files and period number
NIMROD00053344.nxs          SAMPLE  N2 in MCM41 at 88K data files
NIMROD00053345.nxs          SAMPLE  N2 in MCM41 at 88K data files
NIMROD00053346.nxs          SAMPLE  N2 in MCM41 at 88K data files
NIMROD00053347.nxs          SAMPLE  N2 in MCM41 at 88K data files
NIMROD00053352.nxs          SAMPLE  N2 in MCM41 at 88K data files
NIMROD00053353.nxs          SAMPLE  N2 in MCM41 at 88K data files
NIMROD00053354.nxs          SAMPLE  N2 in MCM41 at 88K data files
NIMROD00053355.nxs          SAMPLE  N2 in MCM41 at 88K data files
NIMROD00053356.nxs          SAMPLE  N2 in MCM41 at 88K data files
1          Force calculation of sample corrections?
Si  0  1.0          Composition
O  0  2.11          Composition
H  0  0.22          Composition
N  0  1.499          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.1  0.1          Upstream and downstream thicknesses [cm]
0  10          Angle of rotation and sample width (cm)
-0.03603          Density atoms/Å^3?
0          Temperature for Placzek correction:
TABLES          Total cross section source
5.45          Tweak factor
-10.0          Top hat width (1/Å) for cleaning up Fourier Transform
0.7          Minimum radius for FT  [Å]
0.08          g(r) broadening at r = 1A [A]
0  0          0   0          to finish specifying wavelength range of resonance
0.0  1.0  0          Exponential amplitude and decay [1/A]
*  0  0          * 0 0 to specify end of exponential parameter input
1.0          Normalisation correction factor
NIMROD00053344.msubw01          Name of file containing self scattering as a function of wavelength [A]
0          Normalise to:Nothing
20.0          Maximum radius for FT [A]
0          Output units: b/atom/sr
0.05          Power for broadening function e.g. 0.5
0.03          Step size [A] 
1          Analyse this sample? 
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

CONTAINER 2mm TiZr flat plate cell          {

1  1          Number of  files and period number
NIMROD00053329.nxs          CONTAINER 2mm TiZr flat plate cell data files
Ti  0  7.16          Composition
Zr  0  3.438          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.1  0.1          Upstream and downstream thicknesses [cm]
0  10          Angle of rotation and sample width (cm)
-0.0542          Density atoms/Å^3?
TRANSMISSION          Total cross section source
1.0          Tweak factor
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

GO          

SAMPLE  N2 in MCM41 at 86K          {

14  1          Number of  files and period number
NIMROD00053358.nxs          SAMPLE  N2 in MCM41 at 86K data files
NIMROD00053359.nxs          SAMPLE  N2 in MCM41 at 86K data files
NIMROD00053360.nxs          SAMPLE  N2 in MCM41 at 86K data files
NIMROD00053361.nxs          SAMPLE  N2 in MCM41 at 86K data files
NIMROD00053362.nxs          SAMPLE  N2 in MCM41 at 86K data files
NIMROD00053363.nxs          SAMPLE  N2 in MCM41 at 86K data files
NIMROD00053364.nxs          SAMPLE  N2 in MCM41 at 86K data files
NIMROD00053365.nxs          SAMPLE  N2 in MCM41 at 86K data files
NIMROD00053366.nxs          SAMPLE  N2 in MCM41 at 86K data files
NIMROD00053367.nxs          SAMPLE  N2 in MCM41 at 86K data files
NIMROD00053368.nxs          SAMPLE  N2 in MCM41 at 86K data files
NIMROD00053369.nxs          SAMPLE  N2 in MCM41 at 86K data files
NIMROD00053370.nxs          SAMPLE  N2 in MCM41 at 86K data files
NIMROD00053371.nxs          SAMPLE  N2 in MCM41 at 86K data files
1          Force calculation of sample corrections?
Si  0  1.0          Composition
O  0  2.11          Composition
H  0  0.22          Composition
N  0  1.747          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.1  0.1          Upstream and downstream thicknesses [cm]
0  10          Angle of rotation and sample width (cm)
-0.03788          Density atoms/Å^3?
0          Temperature for Placzek correction:
TABLES          Total cross section source
5.45          Tweak factor
-10.0          Top hat width (1/Å) for cleaning up Fourier Transform
0.7          Minimum radius for FT  [Å]
0.08          g(r) broadening at r = 1A [A]
0  0          0   0          to finish specifying wavelength range of resonance
0.0  1.0  0          Exponential amplitude and decay [1/A]
*  0  0          * 0 0 to specify end of exponential parameter input
1.0          Normalisation correction factor
NIMROD00053358.msubw01          Name of file containing self scattering as a function of wavelength [A]
0          Normalise to:Nothing
20.0          Maximum radius for FT [A]
0          Output units: b/atom/sr
0.05          Power for broadening function e.g. 0.5
0.03          Step size [A] 
1          Analyse this sample? 
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

CONTAINER 2mm TiZr flat plate cell          {

1  1          Number of  files and period number
NIMROD00053329.nxs          CONTAINER 2mm TiZr flat plate cell data files
Ti  0  7.16          Composition
Zr  0  3.438          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.1  0.1          Upstream and downstream thicknesses [cm]
0  10          Angle of rotation and sample width (cm)
-0.0542          Density atoms/Å^3?
TRANSMISSION          Total cross section source
1.0          Tweak factor
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

GO          

SAMPLE  N2 in MCM41 at 85K          {

24  1          Number of  files and period number
NIMROD00053373.nxs          SAMPLE  N2 in MCM41 at 85K data files
NIMROD00053374.nxs          SAMPLE  N2 in MCM41 at 85K data files
NIMROD00053375.nxs          SAMPLE  N2 in MCM41 at 85K data files
NIMROD00053376.nxs          SAMPLE  N2 in MCM41 at 85K data files
NIMROD00053377.nxs          SAMPLE  N2 in MCM41 at 85K data files
NIMROD00053378.nxs          SAMPLE  N2 in MCM41 at 85K data files
NIMROD00053379.nxs          SAMPLE  N2 in MCM41 at 85K data files
NIMROD00053380.nxs          SAMPLE  N2 in MCM41 at 85K data files
NIMROD00053383.nxs          SAMPLE  N2 in MCM41 at 85K data files
NIMROD00053384.nxs          SAMPLE  N2 in MCM41 at 85K data files
NIMROD00053385.nxs          SAMPLE  N2 in MCM41 at 85K data files
NIMROD00053386.nxs          SAMPLE  N2 in MCM41 at 85K data files
NIMROD00053387.nxs          SAMPLE  N2 in MCM41 at 85K data files
NIMROD00053388.nxs          SAMPLE  N2 in MCM41 at 85K data files
NIMROD00053391.nxs          SAMPLE  N2 in MCM41 at 85K data files
NIMROD00053392.nxs          SAMPLE  N2 in MCM41 at 85K data files
NIMROD00053393.nxs          SAMPLE  N2 in MCM41 at 85K data files
NIMROD00053394.nxs          SAMPLE  N2 in MCM41 at 85K data files
NIMROD00053395.nxs          SAMPLE  N2 in MCM41 at 85K data files
NIMROD00053396.nxs          SAMPLE  N2 in MCM41 at 85K data files
NIMROD00053397.nxs          SAMPLE  N2 in MCM41 at 85K data files
NIMROD00053398.nxs          SAMPLE  N2 in MCM41 at 85K data files
NIMROD00053399.nxs          SAMPLE  N2 in MCM41 at 85K data files
NIMROD00053400.nxs          SAMPLE  N2 in MCM41 at 85K data files
1          Force calculation of sample corrections?
Si  0  1.0          Sample atomic composition
O  0  2.11          Sample atomic composition
H  0  0.22          Sample atomic composition
N  0  1.984          Sample atomic composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.1  0.1          Upstream and downstream thicknesses [cm]
0  10          Angle of rotation and sample width (cm)
-0.03965          Density atoms/Å^3?
0          Temperature for sample Placzek correction
TABLES          Total cross section source
5.45          Sample tweak factor
-10.0          Top hat width (1/Å) for cleaning up Fourier Transform
0.7          Minimum radius for FT  [Å]
0.08          g(r) broadening at r = 1A [A]
0  0          0   0          to finish specifying wavelength range of resonance
0.0  1.0  0          Exponential amplitude and decay [1/A]
*  0  0          * 0 0 to specify end of exponential parameter input
1.0          Normalisation correction factor
NIMROD00053373.msubw01          Name of file containing self scattering as a function of wavelength [A]
0          Normalise to:Nothing
20.0          Maximum radius for FT [A]
0          Output units: b/atom/sr
0.05          Power for broadening function e.g. 0.5
0.03          Step size [A] 
1          Analyse this sample? 
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

CONTAINER 2mm TiZr flat plate cell          {

1  1          Number of  files and period number
NIMROD00053329.nxs          CONTAINER 2mm TiZr flat plate cell data files
Ti  0  7.16          Composition
Zr  0  3.438          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.1  0.1          Upstream and downstream thicknesses [cm]
0  10          Angle of rotation and sample width (cm)
-0.0542          Density atoms/Å^3?
TRANSMISSION          Total cross section source
1.0          Tweak factor
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

GO          


END          
1
Date and time last written:  20210305 23:07:44          
N