'  '  '          '  '\'

INSTRUMENT          {

SANDALS          Instrument name
C:\Gudrun_05-06-2019\run\SLS\cycle_24_4\Alderman\          Gudrun input file directory:
Y:\cycle_24_4\          Data file directory
raw          Data file type
StartupFiles\SLS\SANDALS34modulesOct2023_Si.calib          Detector calibration file name
4          User table column number for phi values
StartupFiles\SLS\groups_18.dat          Groups file name
StartupFiles\SLS\SLSdeadtime_35us_Oct2023.cor          Deadtime constants file name
3 4          Spectrum number(s) for incident beam monitor
0  0          Wavelength range [Å] for monitor normalisation
5          Spectrum number(s) for transmission monitor
0.0006          Incident monitor quiet count constant
0.0006          Transmission monitor quiet count constant
0  0          Channel numbers for spike analysis
5          Spike analysis acceptance factor
0.05  4.95  0.1          Wavelength range to use [Å] and step size
100            No. of smooths on monitor
0.1  35.0  0.01          Min, Max and step in x-scale (-ve for logarithmic binning)
0  0  0  0          0 0 0 0 to end input of specified values
1.0          Groups acceptance factor 
4          Merge power
0          Subtract single atom scattering?
2          By channel?
11.016          Incident flight path [m]
0          Spectrum number to output diagnostic files
StartupFiles\SLS\sears91_gudrun.dat          Neutron scattering parameters file
1          Scale selection: 1 = Q, 2 = d-space, 3 = wavelength, 4 = energy, 5 = TOF
0          Subtract wavelength-binned data?
C:\Gudrun_05-06-2019          Folder where Gudrun started
C:\Gudrun_05-06-2019\StartupFiles\SLS          Folder containing the startup file
0.1          Logarithmic step size
1          Hard group edges?
1          Number of iterations
0          Tweak the tweak factor(s)?

}

BEAM          {

CYLINDRICAL          Sample geometry
2          Number of beam profile values
1.0  1.0            Beam profile values (Maximum of 50 allowed currently)
0.05  0.2  100          Step size for absorption and m.s. calculation and no. of slices
10          Angular step for corrections [deg.]          
-1.5  1.5  -1.5  1.5          Incident beam edges relative to centre of sample [cm]
-2.0  2.0  -2.1  2.1          Scattered beam edges relative to centre of sample [cm]
StartupFiles\SLS\spectrum000.dat          Filename containing incident beam spectrum parameters
1.0          Overall background factor 
0.0          Sample dependent background factor
0.0          Shielding attenuation coefficient [per m per A] 

}

NORMALISATION          {

2  1          Number of  files and period number
SLS76999.raw          Data files
SLS77000.raw          Data files
3  1          Number of  files and period number
SLS76993.raw          Data files
SLS76994.raw          Data files
SLS76995.raw          Data files
1          Force calculation of corrections?
V  0  94.85          Composition
Nb  0  5.15          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.0  0.4          Inner and outer radii (cm)
5          Sample height (cm)
-0.071          Density atoms/Å^3?
300          Temperature for Placzek correction:
TABLES          Total cross section source
*          Normalisation differential cross section filename
0.01          Lower limit on smoothed normalisation  
1.05          Normalisation degree of smoothing
0.0          Minimum normalisation signal to background ratio

}

SAMPLE BACKGROUND          {

3  1          Number of  files and period number
SLS76993.raw          SAMPLE BACKGROUND data files
SLS76994.raw          SAMPLE BACKGROUND data files
SLS76995.raw          SAMPLE BACKGROUND data files

}

SAMPLE BBS352 glass          {

8  1          Number of  files and period number
SLS76985.raw          SAMPLE BBS352 glass data files
SLS76986.raw          SAMPLE BBS352 glass data files
SLS76987.raw          SAMPLE BBS352 glass data files
SLS76988.raw          SAMPLE BBS352 glass data files
SLS76989.raw          SAMPLE BBS352 glass data files
SLS76990.raw          SAMPLE BBS352 glass data files
SLS76991.raw          SAMPLE BBS352 glass data files
SLS76992.raw          SAMPLE BBS352 glass data files
1          Force calculation of sample corrections?
B  11  95.904          Sample atomic composition
O  0  144.0          Sample atomic composition
B  10  0.096          Sample atomic composition
Ba  0  28.0          Sample atomic composition
O  0  28.0          Sample atomic composition
Si  0  24.0          Sample atomic composition
O  0  48.0          Sample atomic composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.0  0.55          Inner and outer radii (cm)
5          Sample height (cm)
3.4529          Density Units:  gm/cm^3?
200          Temperature for sample Placzek correction
TRANSMISSION          Total cross section source
2.86071          Sample tweak factor
4.0          Top hat width (1/Å) for cleaning up Fourier Transform
0.3          Minimum radius for FT  [Å]
0.03          g(r) broadening at r = 1A [A]
0  0          0   0          to finish specifying wavelength range of resonance
0.0  1.0  0          Exponential amplitude and decay [1/A]
*  0  0          * 0 0 to specify end of exponential parameter input
1.0          Normalisation correction factor
*          Name of file containing self scattering as a function of wavelength [A]
0          Normalise to:Nothing
20.0          Maximum radius for FT [A]
0          Output units: b/atom/sr
0.0          Power for broadening function e.g. 0.5
0.01          Step size [A] 
0          Analyse this sample? 
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

CONTAINER 11mm drawn vanadium Cylinder          {

3  1          Number of  files and period number
SLS76996.raw          CONTAINER 11mm drawn vanadium Cylinder data files
SLS76997.raw          CONTAINER 11mm drawn vanadium Cylinder data files
SLS76998.raw          CONTAINER 11mm drawn vanadium Cylinder data files
V  0  1.0          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.55  0.563          Inner and outer radii (cm)
5          Sample height (cm)
-0.0721          Density atoms/Å^3?
TRANSMISSION          Total cross section source
1.0          Tweak factor
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

GO          

SAMPLE 11mm drawn vanadium Cylinder          {

3  1          Number of  files and period number
SLS76996.raw          SAMPLE 11mm drawn vanadium Cylinder data files
SLS76997.raw          SAMPLE 11mm drawn vanadium Cylinder data files
SLS76998.raw          SAMPLE 11mm drawn vanadium Cylinder data files
1          Force calculation of sample corrections?
V  0  1.0          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.55  0.563          Inner and outer radii (cm)
5          Sample height (cm)
-0.0721          Density atoms/Å^3?
200          Temperature for Placzek correction:
TRANSMISSION          Total cross section source
1.0          Tweak factor
4.0          Top hat width (1/Å) for cleaning up Fourier Transform
0.3          Minimum radius for FT  [Å]
0.03          g(r) broadening at r = 1A [A]
0  0          0   0          to finish specifying wavelength range of resonance
0.0  1.0  0          Exponential amplitude and decay [1/A]
*  0  0          * 0 0 to specify end of exponential parameter input
1.0          Normalisation correction factor
*          Name of file containing self scattering as a function of wavelength [A]
0          Normalise to:Nothing
20.0          Maximum radius for FT [A]
0          Output units: b/atom/sr
0.0          Power for broadening function e.g. 0.5
0.01          Step size [A] 
0          Analyse this sample? 
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

GO          

SAMPLE G0 glass          {

9  1          Number of  files and period number
SLS77001.raw          SAMPLE G0 glass data files
SLS77002.raw          SAMPLE G0 glass data files
SLS77003.raw          SAMPLE G0 glass data files
SLS77004.raw          SAMPLE G0 glass data files
SLS77005.raw          SAMPLE G0 glass data files
SLS77006.raw          SAMPLE G0 glass data files
SLS77007.raw          SAMPLE G0 glass data files
SLS77008.raw          SAMPLE G0 glass data files
SLS77009.raw          SAMPLE G0 glass data files
1          Force calculation of sample corrections?
B  11  49.95          Sample atomic composition
O  0  75.0          Sample atomic composition
B  10  0.05          Sample atomic composition
Ba  0  50.0          Sample atomic composition
O  0  50.0          Sample atomic composition
Si  0  25.0          Sample atomic composition
O  0  50.0          Sample atomic composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.0  0.55          Inner and outer radii (cm)
5          Sample height (cm)
4.2167          Density Units:  gm/cm^3?
200          Temperature for sample Placzek correction
TRANSMISSION          Total cross section source
2.14057          Sample tweak factor
4.0          Top hat width (1/Å) for cleaning up Fourier Transform
0.3          Minimum radius for FT  [Å]
0.03          g(r) broadening at r = 1A [A]
0  0          0   0          to finish specifying wavelength range of resonance
0.0  1.0  0          Exponential amplitude and decay [1/A]
*  0  0          * 0 0 to specify end of exponential parameter input
1.0          Normalisation correction factor
*          Name of file containing self scattering as a function of wavelength [A]
0          Normalise to:Nothing
20.0          Maximum radius for FT [A]
0          Output units: b/atom/sr
0.0          Power for broadening function e.g. 0.5
0.01          Step size [A] 
1          Analyse this sample? 
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

CONTAINER 11mm drawn vanadium Cylinder          {

3  1          Number of  files and period number
SLS76996.raw          CONTAINER 11mm drawn vanadium Cylinder data files
SLS76997.raw          CONTAINER 11mm drawn vanadium Cylinder data files
SLS76998.raw          CONTAINER 11mm drawn vanadium Cylinder data files
V  0  1.0          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.55  0.563          Inner and outer radii (cm)
5          Sample height (cm)
-0.0721          Density atoms/Å^3?
TRANSMISSION          Total cross section source
1.0          Tweak factor
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

GO          


END          
1 2 3 4 5 6 7 8 9 10
Date and time last written:  20250226 13:57:07          
N