'  '  '          '  '\'

INSTRUMENT          {

SANDALS          Instrument name
C:\Gudrun_05-06-2019\run\SLS\cycle_24_4\Alderman\          Gudrun input file directory:
Y:\cycle_24_4\          Data file directory
raw          Data file type
StartupFiles\SLS\SANDALS34modulesOct2023_Si.calib          Detector calibration file name
4          User table column number for phi values
StartupFiles\SLS\groups_18.dat          Groups file name
StartupFiles\SLS\SLSdeadtime_35us_Oct2023.cor          Deadtime constants file name
3 4          Spectrum number(s) for incident beam monitor
0  0          Wavelength range [Å] for monitor normalisation
5          Spectrum number(s) for transmission monitor
0.0006          Incident monitor quiet count constant
0.0006          Transmission monitor quiet count constant
0  0          Channel numbers for spike analysis
5          Spike analysis acceptance factor
0.09  4.95  0.1          Wavelength range to use [Å] and step size
100            No. of smooths on monitor
0.1  35.0  0.01          Min, Max and step in x-scale (-ve for logarithmic binning)
0  0  0  0          0 0 0 0 to end input of specified values
1.0          Groups acceptance factor 
4          Merge power
0          Subtract single atom scattering?
2          By channel?
11.016          Incident flight path [m]
0          Spectrum number to output diagnostic files
StartupFiles\SLS\sears91_gudrun.dat          Neutron scattering parameters file
1          Scale selection: 1 = Q, 2 = d-space, 3 = wavelength, 4 = energy, 5 = TOF
0          Subtract wavelength-binned data?
C:\Gudrun_05-06-2019          Folder where Gudrun started
C:\Gudrun_05-06-2019\StartupFiles\SLS          Folder containing the startup file
0.1          Logarithmic step size
1          Hard group edges?
1          Number of iterations
0          Tweak the tweak factor(s)?

}

BEAM          {

CYLINDRICAL          Sample geometry
2          Number of beam profile values
1.0  1.0            Beam profile values (Maximum of 50 allowed currently)
0.05  0.2  100          Step size for absorption and m.s. calculation and no. of slices
10          Angular step for corrections [deg.]          
-0.425  0.425  -1.5  1.5          Incident beam edges relative to centre of sample [cm]
-0.6  0.6  -2.1  2.1          Scattered beam edges relative to centre of sample [cm]
StartupFiles\SLS\spectrum000.dat          Filename containing incident beam spectrum parameters
1.0          Overall background factor 
0.0          Sample dependent background factor
0.0          Shielding attenuation coefficient [per m per A] 

}

NORMALISATION          {

2  1          Number of  files and period number
SLS76999.raw          Data files
SLS77000.raw          Data files
3  1          Number of  files and period number
SLS76993.raw          Data files
SLS76994.raw          Data files
SLS76995.raw          Data files
1          Force calculation of corrections?
V  0  94.85          Composition
Nb  0  5.15          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.0  0.4          Inner and outer radii (cm)
5          Sample height (cm)
-0.071          Density atoms/Å^3?
300          Temperature for Placzek correction:
TABLES          Total cross section source
*          Normalisation differential cross section filename
0.01          Lower limit on smoothed normalisation  
1.05          Normalisation degree of smoothing
0.0          Minimum normalisation signal to background ratio

}

SAMPLE BACKGROUND          {

3  1          Number of  files and period number
SLS76993.raw          SAMPLE BACKGROUND data files
SLS76994.raw          SAMPLE BACKGROUND data files
SLS76995.raw          SAMPLE BACKGROUND data files

}

SAMPLE BBS352 glass          {

8  1          Number of  files and period number
SLS76985.raw          SAMPLE BBS352 glass data files
SLS76986.raw          SAMPLE BBS352 glass data files
SLS76987.raw          SAMPLE BBS352 glass data files
SLS76988.raw          SAMPLE BBS352 glass data files
SLS76989.raw          SAMPLE BBS352 glass data files
SLS76990.raw          SAMPLE BBS352 glass data files
SLS76991.raw          SAMPLE BBS352 glass data files
SLS76992.raw          SAMPLE BBS352 glass data files
1          Force calculation of sample corrections?
B  11  95.904          Composition
O  0  144.0          Composition
B  10  0.096          Composition
Ba  0  28.0          Composition
O  0  28.0          Composition
Si  0  24.0          Composition
O  0  48.0          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.0  0.55          Inner and outer radii (cm)
5          Sample height (cm)
3.4529          Density Units:  gm/cm^3?
200          Temperature for Placzek correction:
TRANSMISSION          Total cross section source
2.86071          Tweak factor
4.0          Top hat width (1/Å) for cleaning up Fourier Transform
0.3          Minimum radius for FT  [Å]
0.03          g(r) broadening at r = 1A [A]
0  0          0   0          to finish specifying wavelength range of resonance
0.0  1.0  0          Exponential amplitude and decay [1/A]
*  0  0          * 0 0 to specify end of exponential parameter input
1.0          Normalisation correction factor
*          Name of file containing self scattering as a function of wavelength [A]
0          Normalise to:Nothing
20.0          Maximum radius for FT [A]
0          Output units: b/atom/sr
0.0          Power for broadening function e.g. 0.5
0.01          Step size [A] 
0          Analyse this sample? 
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

CONTAINER 11mm drawn vanadium Cylinder          {

3  1          Number of  files and period number
SLS76996.raw          CONTAINER 11mm drawn vanadium Cylinder data files
SLS76997.raw          CONTAINER 11mm drawn vanadium Cylinder data files
SLS76998.raw          CONTAINER 11mm drawn vanadium Cylinder data files
V  0  1.0          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.55  0.563          Inner and outer radii (cm)
5          Sample height (cm)
-0.0721          Density atoms/Å^3?
TRANSMISSION          Total cross section source
1.0          Tweak factor
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

GO          

SAMPLE 11mm drawn vanadium Cylinder          {

3  1          Number of  files and period number
SLS76996.raw          SAMPLE 11mm drawn vanadium Cylinder data files
SLS76997.raw          SAMPLE 11mm drawn vanadium Cylinder data files
SLS76998.raw          SAMPLE 11mm drawn vanadium Cylinder data files
1          Force calculation of sample corrections?
V  0  1.0          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.55  0.563          Inner and outer radii (cm)
5          Sample height (cm)
-0.0721          Density atoms/Å^3?
200          Temperature for Placzek correction:
TRANSMISSION          Total cross section source
1.0          Tweak factor
4.0          Top hat width (1/Å) for cleaning up Fourier Transform
0.3          Minimum radius for FT  [Å]
0.03          g(r) broadening at r = 1A [A]
0  0          0   0          to finish specifying wavelength range of resonance
0.0  1.0  0          Exponential amplitude and decay [1/A]
*  0  0          * 0 0 to specify end of exponential parameter input
1.0          Normalisation correction factor
*          Name of file containing self scattering as a function of wavelength [A]
0          Normalise to:Nothing
20.0          Maximum radius for FT [A]
0          Output units: b/atom/sr
0.0          Power for broadening function e.g. 0.5
0.01          Step size [A] 
0          Analyse this sample? 
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

GO          

SAMPLE G0 glass          {

9  1          Number of  files and period number
SLS77001.raw          SAMPLE G0 glass data files
SLS77002.raw          SAMPLE G0 glass data files
SLS77003.raw          SAMPLE G0 glass data files
SLS77004.raw          SAMPLE G0 glass data files
SLS77005.raw          SAMPLE G0 glass data files
SLS77006.raw          SAMPLE G0 glass data files
SLS77007.raw          SAMPLE G0 glass data files
SLS77008.raw          SAMPLE G0 glass data files
SLS77009.raw          SAMPLE G0 glass data files
1          Force calculation of sample corrections?
B  11  49.95          Composition
O  0  75.0          Composition
B  10  0.05          Composition
Ba  0  50.0          Composition
O  0  50.0          Composition
Si  0  25.0          Composition
O  0  50.0          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.0  0.55          Inner and outer radii (cm)
5          Sample height (cm)
4.2167          Density Units:  gm/cm^3?
200          Temperature for Placzek correction:
TRANSMISSION          Total cross section source
2.14057          Tweak factor
4.0          Top hat width (1/Å) for cleaning up Fourier Transform
0.3          Minimum radius for FT  [Å]
0.03          g(r) broadening at r = 1A [A]
0  0          0   0          to finish specifying wavelength range of resonance
0.0  1.0  0          Exponential amplitude and decay [1/A]
*  0  0          * 0 0 to specify end of exponential parameter input
1.0          Normalisation correction factor
*          Name of file containing self scattering as a function of wavelength [A]
0          Normalise to:Nothing
20.0          Maximum radius for FT [A]
0          Output units: b/atom/sr
0.0          Power for broadening function e.g. 0.5
0.01          Step size [A] 
0          Analyse this sample? 
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

CONTAINER 11mm drawn vanadium Cylinder          {

3  1          Number of  files and period number
SLS76996.raw          CONTAINER 11mm drawn vanadium Cylinder data files
SLS76997.raw          CONTAINER 11mm drawn vanadium Cylinder data files
SLS76998.raw          CONTAINER 11mm drawn vanadium Cylinder data files
V  0  1.0          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.55  0.563          Inner and outer radii (cm)
5          Sample height (cm)
-0.0721          Density atoms/Å^3?
TRANSMISSION          Total cross section source
1.0          Tweak factor
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

GO          

SAMPLE BBS352 glass          {

8  1          Number of  files and period number
SLS77146.raw          SAMPLE BBS352 glass data files
SLS77147.raw          SAMPLE BBS352 glass data files
SLS77148.raw          SAMPLE BBS352 glass data files
SLS77149.raw          SAMPLE BBS352 glass data files
SLS77150.raw          SAMPLE BBS352 glass data files
SLS77151.raw          SAMPLE BBS352 glass data files
SLS77152.raw          SAMPLE BBS352 glass data files
SLS77153.raw          SAMPLE BBS352 glass data files
1          Force calculation of sample corrections?
V  0  1.0          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.0  0.3          Inner and outer radii (cm)
5          Sample height (cm)
-0.071          Density atoms/Å^3?
866.67          Temperature for Placzek correction:
TRANSMISSION          Total cross section source
2.353          Tweak factor
4.0          Top hat width (1/Å) for cleaning up Fourier Transform
0.3          Minimum radius for FT  [Å]
0.03          g(r) broadening at r = 1A [A]
0  0          0   0          to finish specifying wavelength range of resonance
0.0  1.0  0          Exponential amplitude and decay [1/A]
*  0  0          * 0 0 to specify end of exponential parameter input
1.0          Normalisation correction factor
*          Name of file containing self scattering as a function of wavelength [A]
0          Normalise to:Nothing
20.0          Maximum radius for FT [A]
0          Output units: b/atom/sr
0.0          Power for broadening function e.g. 0.5
0.01          Step size [A] 
0          Analyse this sample? 
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

GO          

SAMPLE BACKGROUND          {

3  1          Number of  files and period number
SLS77055.raw          SAMPLE BACKGROUND data files
SLS77056.raw          SAMPLE BACKGROUND data files
SLS77057.raw          SAMPLE BACKGROUND data files

}

SAMPLE 11mm Pt 27C          {

2  1          Number of  files and period number
SLS77017.raw          SAMPLE 11mm Pt 27C data files
SLS77018.raw          SAMPLE 11mm Pt 27C data files
1          Force calculation of sample corrections?
Pt  0  1.0          Sample atomic composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.537  0.55          Inner and outer radii (cm)
5          Sample height (cm)
21.45          Density Units:  gm/cm^3?
200          Temperature for sample Placzek correction
TRANSMISSION          Total cross section source
1.0          Sample tweak factor
4.0          Top hat width (1/Å) for cleaning up Fourier Transform
0.3          Minimum radius for FT  [Å]
0.03          g(r) broadening at r = 1A [A]
0  0          0   0          to finish specifying wavelength range of resonance
0.0  1.0  0          Exponential amplitude and decay [1/A]
*  0  0          * 0 0 to specify end of exponential parameter input
1.0          Normalisation correction factor
*          Name of file containing self scattering as a function of wavelength [A]
0          Normalise to:Nothing
20.0          Maximum radius for FT [A]
0          Output units: b/atom/sr
0.0          Power for broadening function e.g. 0.5
0.01          Step size [A] 
0          Analyse this sample? 
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

GO          

SAMPLE 11mm Pt 327C          {

2  1          Number of  files and period number
SLS77028.raw          SAMPLE 11mm Pt 327C data files
SLS77029.raw          SAMPLE 11mm Pt 327C data files
1          Force calculation of sample corrections?
Pt  0  1.0          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.537  0.55          Inner and outer radii (cm)
5          Sample height (cm)
21.268          Density Units:  gm/cm^3?
400          Temperature for Placzek correction:
TABLES          Total cross section source
1.0          Tweak factor
4.0          Top hat width (1/Å) for cleaning up Fourier Transform
0.3          Minimum radius for FT  [Å]
0.03          g(r) broadening at r = 1A [A]
0  0          0   0          to finish specifying wavelength range of resonance
0.0  1.0  0          Exponential amplitude and decay [1/A]
*  0  0          * 0 0 to specify end of exponential parameter input
1.0          Normalisation correction factor
*          Name of file containing self scattering as a function of wavelength [A]
0          Normalise to:Nothing
20.0          Maximum radius for FT [A]
0          Output units: b/atom/sr
0.0          Power for broadening function e.g. 0.5
0.01          Step size [A] 
0          Analyse this sample? 
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

GO          

SAMPLE 11mm Pt 1027C          {

2  1          Number of  files and period number
SLS77049.raw          SAMPLE 11mm Pt 1027C data files
SLS77050.raw          SAMPLE 11mm Pt 1027C data files
1          Force calculation of sample corrections?
Pt  0  1.0          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.537  0.55          Inner and outer radii (cm)
5          Sample height (cm)
20.797          Density Units:  gm/cm^3?
866.67          Temperature for Placzek correction:
TRANSMISSION          Total cross section source
1.0          Tweak factor
4.0          Top hat width (1/Å) for cleaning up Fourier Transform
0.3          Minimum radius for FT  [Å]
0.03          g(r) broadening at r = 1A [A]
0  0          0   0          to finish specifying wavelength range of resonance
0.0  1.0  0          Exponential amplitude and decay [1/A]
*  0  0          * 0 0 to specify end of exponential parameter input
1.0          Normalisation correction factor
*          Name of file containing self scattering as a function of wavelength [A]
0          Normalise to:Nothing
20.0          Maximum radius for FT [A]
0          Output units: b/atom/sr
0.0          Power for broadening function e.g. 0.5
0.01          Step size [A] 
0          Analyse this sample? 
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

GO          

SAMPLE 11mm Pt 1127C          {

2  1          Number of  files and period number
SLS77052.raw          SAMPLE 11mm Pt 1127C data files
SLS77054.raw          SAMPLE 11mm Pt 1127C data files
1          Force calculation of sample corrections?
Pt  0  1.0          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.537  0.55          Inner and outer radii (cm)
5          Sample height (cm)
20.72          Density Units:  gm/cm^3?
933          Temperature for Placzek correction:
TRANSMISSION          Total cross section source
1.0          Tweak factor
4.0          Top hat width (1/Å) for cleaning up Fourier Transform
0.3          Minimum radius for FT  [Å]
0.03          g(r) broadening at r = 1A [A]
0  0          0   0          to finish specifying wavelength range of resonance
0.0  1.0  0          Exponential amplitude and decay [1/A]
*  0  0          * 0 0 to specify end of exponential parameter input
1.0          Normalisation correction factor
*          Name of file containing self scattering as a function of wavelength [A]
0          Normalise to:Nothing
20.0          Maximum radius for FT [A]
0          Output units: b/atom/sr
0.0          Power for broadening function e.g. 0.5
0.01          Step size [A] 
0          Analyse this sample? 
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

GO          

SAMPLE BBS352 glass          {

4  1          Number of  files and period number
SLS77058.raw          SAMPLE BBS352 glass data files
SLS77059.raw          SAMPLE BBS352 glass data files
SLS77060.raw          SAMPLE BBS352 glass data files
SLS77061.raw          SAMPLE BBS352 glass data files
1          Force calculation of sample corrections?
B  11  95.904          Sample atomic composition
O  0  144.0          Sample atomic composition
B  10  0.096          Sample atomic composition
Ba  0  28.0          Sample atomic composition
O  0  28.0          Sample atomic composition
Si  0  24.0          Sample atomic composition
O  0  48.0          Sample atomic composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.0  0.55          Inner and outer radii (cm)
5          Sample height (cm)
3.4525          Density Units:  gm/cm^3?
200          Temperature for sample Placzek correction
TRANSMISSION          Total cross section source
2.02276          Sample tweak factor
4.0          Top hat width (1/Å) for cleaning up Fourier Transform
0.3          Minimum radius for FT  [Å]
0.03          g(r) broadening at r = 1A [A]
0  0          0   0          to finish specifying wavelength range of resonance
0.0  1.0  0          Exponential amplitude and decay [1/A]
*  0  0          * 0 0 to specify end of exponential parameter input
1.0          Normalisation correction factor
*          Name of file containing self scattering as a function of wavelength [A]
0          Normalise to:Nothing
20.0          Maximum radius for FT [A]
0          Output units: b/atom/sr
0.0          Power for broadening function e.g. 0.5
0.01          Step size [A] 
0          Analyse this sample? 
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

CONTAINER 11mm Pt 27C          {

2  1          Number of  files and period number
SLS77017.raw          CONTAINER 11mm Pt 27C data files
SLS77018.raw          CONTAINER 11mm Pt 27C data files
Pt  0  1.0          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.537  0.55          Inner and outer radii (cm)
5          Sample height (cm)
21.45          Density Units:  gm/cm^3?
TRANSMISSION          Total cross section source
0.95          Tweak factor
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

GO          

SAMPLE BBS352 glass          {

4  1          Number of  files and period number
SLS77064.raw          SAMPLE BBS352 glass data files
SLS77065.raw          SAMPLE BBS352 glass data files
SLS77066.raw          SAMPLE BBS352 glass data files
SLS77067.raw          SAMPLE BBS352 glass data files
1          Force calculation of sample corrections?
B  11  95.904          Sample atomic composition
O  0  144.0          Sample atomic composition
B  10  0.096          Sample atomic composition
Ba  0  28.0          Sample atomic composition
O  0  28.0          Sample atomic composition
Si  0  24.0          Sample atomic composition
O  0  48.0          Sample atomic composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.0  0.55          Inner and outer radii (cm)
5          Sample height (cm)
3.446154037          Density Units:  gm/cm^3?
266.67          Temperature for sample Placzek correction
TRANSMISSION          Total cross section source
2.02778          Sample tweak factor
4.0          Top hat width (1/Å) for cleaning up Fourier Transform
0.3          Minimum radius for FT  [Å]
0.03          g(r) broadening at r = 1A [A]
0  0          0   0          to finish specifying wavelength range of resonance
0.0  1.0  0          Exponential amplitude and decay [1/A]
*  0  0          * 0 0 to specify end of exponential parameter input
1.0          Normalisation correction factor
*          Name of file containing self scattering as a function of wavelength [A]
0          Normalise to:Nothing
20.0          Maximum radius for FT [A]
0          Output units: b/atom/sr
0.0          Power for broadening function e.g. 0.5
0.01          Step size [A] 
0          Analyse this sample? 
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

CONTAINER 11mm Pt 127C          {

2  1          Number of  files and period number
SLS77021.raw          CONTAINER 11mm Pt 127C data files
SLS77022.raw          CONTAINER 11mm Pt 127C data files
Pt  0  1.0          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.537  0.55          Inner and outer radii (cm)
5          Sample height (cm)
21.389          Density Units:  gm/cm^3?
TRANSMISSION          Total cross section source
0.95          Tweak factor
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

GO          

SAMPLE BBS352 glass          {

4  1          Number of  files and period number
SLS77070.raw          SAMPLE BBS352 glass data files
SLS77071.raw          SAMPLE BBS352 glass data files
SLS77072.raw          SAMPLE BBS352 glass data files
SLS77073.raw          SAMPLE BBS352 glass data files
1          Force calculation of sample corrections?
B  11  95.904          Sample atomic composition
O  0  144.0          Sample atomic composition
B  10  0.096          Sample atomic composition
Ba  0  28.0          Sample atomic composition
O  0  28.0          Sample atomic composition
Si  0  24.0          Sample atomic composition
O  0  48.0          Sample atomic composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.0  0.55          Inner and outer radii (cm)
5          Sample height (cm)
3.438832409          Density Units:  gm/cm^3?
333.33          Temperature for sample Placzek correction
TRANSMISSION          Total cross section source
2.02525          Sample tweak factor
4.0          Top hat width (1/Å) for cleaning up Fourier Transform
0.3          Minimum radius for FT  [Å]
0.03          g(r) broadening at r = 1A [A]
0  0          0   0          to finish specifying wavelength range of resonance
0.0  1.0  0          Exponential amplitude and decay [1/A]
*  0  0          * 0 0 to specify end of exponential parameter input
1.0          Normalisation correction factor
*          Name of file containing self scattering as a function of wavelength [A]
0          Normalise to:Nothing
20.0          Maximum radius for FT [A]
0          Output units: b/atom/sr
0.0          Power for broadening function e.g. 0.5
0.01          Step size [A] 
0          Analyse this sample? 
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

CONTAINER 11mm Pt 227C          {

2  1          Number of  files and period number
SLS77025.raw          CONTAINER 11mm Pt 227C data files
SLS77026.raw          CONTAINER 11mm Pt 227C data files
Pt  0  1.0          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.537  0.55          Inner and outer radii (cm)
5          Sample height (cm)
21.329          Density Units:  gm/cm^3?
TRANSMISSION          Total cross section source
0.95          Tweak factor
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

GO          

SAMPLE BBS352 glass          {

4  1          Number of  files and period number
SLS77075.raw          SAMPLE BBS352 glass data files
SLS77076.raw          SAMPLE BBS352 glass data files
SLS77077.raw          SAMPLE BBS352 glass data files
SLS77078.raw          SAMPLE BBS352 glass data files
1          Force calculation of sample corrections?
B  11  95.904          Sample atomic composition
O  0  144.0          Sample atomic composition
B  10  0.096          Sample atomic composition
Ba  0  28.0          Sample atomic composition
O  0  28.0          Sample atomic composition
Si  0  24.0          Sample atomic composition
O  0  48.0          Sample atomic composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.0  0.55          Inner and outer radii (cm)
5          Sample height (cm)
3.431787253          Density Units:  gm/cm^3?
400          Temperature for sample Placzek correction
TRANSMISSION          Total cross section source
2.03261          Sample tweak factor
4.0          Top hat width (1/Å) for cleaning up Fourier Transform
0.3          Minimum radius for FT  [Å]
0.03          g(r) broadening at r = 1A [A]
0  0          0   0          to finish specifying wavelength range of resonance
0.0  1.0  0          Exponential amplitude and decay [1/A]
*  0  0          * 0 0 to specify end of exponential parameter input
1.0          Normalisation correction factor
*          Name of file containing self scattering as a function of wavelength [A]
0          Normalise to:Nothing
20.0          Maximum radius for FT [A]
0          Output units: b/atom/sr
0.0          Power for broadening function e.g. 0.5
0.01          Step size [A] 
0          Analyse this sample? 
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

CONTAINER 11mm Pt 327C          {

2  1          Number of  files and period number
SLS77028.raw          CONTAINER 11mm Pt 327C data files
SLS77029.raw          CONTAINER 11mm Pt 327C data files
Pt  0  1.0          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.537  0.55          Inner and outer radii (cm)
5          Sample height (cm)
21.268          Density Units:  gm/cm^3?
TABLES          Total cross section source
0.95          Tweak factor
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

GO          

SAMPLE BBS352 glass          {

10  1          Number of  files and period number
SLS77080.raw          SAMPLE BBS352 glass data files
SLS77081.raw          SAMPLE BBS352 glass data files
SLS77082.raw          SAMPLE BBS352 glass data files
SLS77083.raw          SAMPLE BBS352 glass data files
SLS77084.raw          SAMPLE BBS352 glass data files
SLS77085.raw          SAMPLE BBS352 glass data files
SLS77086.raw          SAMPLE BBS352 glass data files
SLS77087.raw          SAMPLE BBS352 glass data files
SLS77088.raw          SAMPLE BBS352 glass data files
SLS77089.raw          SAMPLE BBS352 glass data files
1          Force calculation of sample corrections?
B  11  95.904          Sample atomic composition
O  0  144.0          Sample atomic composition
B  10  0.096          Sample atomic composition
Ba  0  28.0          Sample atomic composition
O  0  28.0          Sample atomic composition
Si  0  24.0          Sample atomic composition
O  0  48.0          Sample atomic composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.0  0.55          Inner and outer radii (cm)
5          Sample height (cm)
3.424316784          Density Units:  gm/cm^3?
466.67          Temperature for sample Placzek correction
TRANSMISSION          Total cross section source
2.03704          Sample tweak factor
4.0          Top hat width (1/Å) for cleaning up Fourier Transform
0.3          Minimum radius for FT  [Å]
0.03          g(r) broadening at r = 1A [A]
0  0          0   0          to finish specifying wavelength range of resonance
0.0  1.0  0          Exponential amplitude and decay [1/A]
*  0  0          * 0 0 to specify end of exponential parameter input
1.0          Normalisation correction factor
*          Name of file containing self scattering as a function of wavelength [A]
0          Normalise to:Nothing
20.0          Maximum radius for FT [A]
0          Output units: b/atom/sr
0.0          Power for broadening function e.g. 0.5
0.01          Step size [A] 
0          Analyse this sample? 
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

CONTAINER 11mm Pt 427C          {

2  1          Number of  files and period number
SLS77031.raw          CONTAINER 11mm Pt 427C data files
SLS77032.raw          CONTAINER 11mm Pt 427C data files
Pt  0  1.0          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.537  0.55          Inner and outer radii (cm)
5          Sample height (cm)
21.205          Density Units:  gm/cm^3?
TABLES          Total cross section source
0.95          Tweak factor
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

GO          

SAMPLE BBS352 glass          {

10  1          Number of  files and period number
SLS77091.raw          SAMPLE BBS352 glass data files
SLS77092.raw          SAMPLE BBS352 glass data files
SLS77093.raw          SAMPLE BBS352 glass data files
SLS77094.raw          SAMPLE BBS352 glass data files
SLS77095.raw          SAMPLE BBS352 glass data files
SLS77096.raw          SAMPLE BBS352 glass data files
SLS77097.raw          SAMPLE BBS352 glass data files
SLS77098.raw          SAMPLE BBS352 glass data files
SLS77099.raw          SAMPLE BBS352 glass data files
SLS77100.raw          SAMPLE BBS352 glass data files
1          Force calculation of sample corrections?
B  11  95.904          Sample atomic composition
O  0  144.0          Sample atomic composition
B  10  0.096          Sample atomic composition
Ba  0  28.0          Sample atomic composition
O  0  28.0          Sample atomic composition
Si  0  24.0          Sample atomic composition
O  0  48.0          Sample atomic composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.0  0.55          Inner and outer radii (cm)
5          Sample height (cm)
3.420028677          Density Units:  gm/cm^3?
533.33          Temperature for sample Placzek correction
TRANSMISSION          Total cross section source
2.0502          Sample tweak factor
4.0          Top hat width (1/Å) for cleaning up Fourier Transform
0.3          Minimum radius for FT  [Å]
0.03          g(r) broadening at r = 1A [A]
0  0          0   0          to finish specifying wavelength range of resonance
0.0  1.0  0          Exponential amplitude and decay [1/A]
*  0  0          * 0 0 to specify end of exponential parameter input
1.0          Normalisation correction factor
*          Name of file containing self scattering as a function of wavelength [A]
0          Normalise to:Nothing
20.0          Maximum radius for FT [A]
0          Output units: b/atom/sr
0.0          Power for broadening function e.g. 0.5
0.01          Step size [A] 
0          Analyse this sample? 
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

CONTAINER 11mm Pt 527C          {

2  1          Number of  files and period number
SLS77034.raw          CONTAINER 11mm Pt 527C data files
SLS77035.raw          CONTAINER 11mm Pt 527C data files
Pt  0  1.0          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.537  0.55          Inner and outer radii (cm)
5          Sample height (cm)
21.142          Density Units:  gm/cm^3?
TRANSMISSION          Total cross section source
0.95          Tweak factor
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

GO          

SAMPLE BBS352 glass          {

10  1          Number of  files and period number
SLS77102.raw          SAMPLE BBS352 glass data files
SLS77103.raw          SAMPLE BBS352 glass data files
SLS77104.raw          SAMPLE BBS352 glass data files
SLS77105.raw          SAMPLE BBS352 glass data files
SLS77106.raw          SAMPLE BBS352 glass data files
SLS77107.raw          SAMPLE BBS352 glass data files
SLS77108.raw          SAMPLE BBS352 glass data files
SLS77109.raw          SAMPLE BBS352 glass data files
SLS77110.raw          SAMPLE BBS352 glass data files
SLS77111.raw          SAMPLE BBS352 glass data files
1          Force calculation of sample corrections?
B  11  95.904          Sample atomic composition
O  0  144.0          Sample atomic composition
B  10  0.096          Sample atomic composition
Ba  0  28.0          Sample atomic composition
O  0  28.0          Sample atomic composition
Si  0  24.0          Sample atomic composition
O  0  48.0          Sample atomic composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.0  0.55          Inner and outer radii (cm)
5          Sample height (cm)
3.413224686          Density Units:  gm/cm^3?
600          Temperature for sample Placzek correction
TRANSMISSION          Total cross section source
2.06299          Sample tweak factor
4.0          Top hat width (1/Å) for cleaning up Fourier Transform
0.3          Minimum radius for FT  [Å]
0.03          g(r) broadening at r = 1A [A]
0  0          0   0          to finish specifying wavelength range of resonance
0.0  1.0  0          Exponential amplitude and decay [1/A]
*  0  0          * 0 0 to specify end of exponential parameter input
1.0          Normalisation correction factor
*          Name of file containing self scattering as a function of wavelength [A]
0          Normalise to:Nothing
20.0          Maximum radius for FT [A]
0          Output units: b/atom/sr
0.0          Power for broadening function e.g. 0.5
0.01          Step size [A] 
0          Analyse this sample? 
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

CONTAINER 11mm Pt 627C          {

2  1          Number of  files and period number
SLS77037.raw          CONTAINER 11mm Pt 627C data files
SLS77038.raw          CONTAINER 11mm Pt 627C data files
Pt  0  1.0          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.537  0.55          Inner and outer radii (cm)
5          Sample height (cm)
21.076          Density Units:  gm/cm^3?
TRANSMISSION          Total cross section source
0.95          Tweak factor
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

GO          

SAMPLE BBS352 glass          {

10  1          Number of  files and period number
SLS77113.raw          SAMPLE BBS352 glass data files
SLS77114.raw          SAMPLE BBS352 glass data files
SLS77115.raw          SAMPLE BBS352 glass data files
SLS77116.raw          SAMPLE BBS352 glass data files
SLS77117.raw          SAMPLE BBS352 glass data files
SLS77118.raw          SAMPLE BBS352 glass data files
SLS77119.raw          SAMPLE BBS352 glass data files
SLS77120.raw          SAMPLE BBS352 glass data files
SLS77121.raw          SAMPLE BBS352 glass data files
SLS77122.raw          SAMPLE BBS352 glass data files
1          Force calculation of sample corrections?
B  11  95.904          Sample atomic composition
O  0  144.0          Sample atomic composition
B  10  0.096          Sample atomic composition
Ba  0  28.0          Sample atomic composition
O  0  28.0          Sample atomic composition
Si  0  24.0          Sample atomic composition
O  0  48.0          Sample atomic composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.0  0.55          Inner and outer radii (cm)
5          Sample height (cm)
3.299053989          Density Units:  gm/cm^3?
666.67          Temperature for sample Placzek correction
TRANSMISSION          Total cross section source
2.23264          Sample tweak factor
4.0          Top hat width (1/Å) for cleaning up Fourier Transform
0.3          Minimum radius for FT  [Å]
0.03          g(r) broadening at r = 1A [A]
0  0          0   0          to finish specifying wavelength range of resonance
0.0  1.0  0          Exponential amplitude and decay [1/A]
*  0  0          * 0 0 to specify end of exponential parameter input
1.0          Normalisation correction factor
*          Name of file containing self scattering as a function of wavelength [A]
0          Normalise to:Nothing
20.0          Maximum radius for FT [A]
0          Output units: b/atom/sr
0.0          Power for broadening function e.g. 0.5
0.01          Step size [A] 
0          Analyse this sample? 
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

CONTAINER 11mm Pt 727C          {

2  1          Number of  files and period number
SLS77040.raw          CONTAINER 11mm Pt 727C data files
SLS77041.raw          CONTAINER 11mm Pt 727C data files
Pt  0  1.0          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.537  0.55          Inner and outer radii (cm)
5          Sample height (cm)
21.009          Density Units:  gm/cm^3?
TRANSMISSION          Total cross section source
0.95          Tweak factor
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

GO          

SAMPLE BBS352 glass          {

10  1          Number of  files and period number
SLS77124.raw          SAMPLE BBS352 glass data files
SLS77125.raw          SAMPLE BBS352 glass data files
SLS77126.raw          SAMPLE BBS352 glass data files
SLS77127.raw          SAMPLE BBS352 glass data files
SLS77128.raw          SAMPLE BBS352 glass data files
SLS77129.raw          SAMPLE BBS352 glass data files
SLS77130.raw          SAMPLE BBS352 glass data files
SLS77131.raw          SAMPLE BBS352 glass data files
SLS77132.raw          SAMPLE BBS352 glass data files
SLS77133.raw          SAMPLE BBS352 glass data files
1          Force calculation of sample corrections?
B  11  95.904          Sample atomic composition
O  0  144.0          Sample atomic composition
B  10  0.096          Sample atomic composition
Ba  0  28.0          Sample atomic composition
O  0  28.0          Sample atomic composition
Si  0  24.0          Sample atomic composition
O  0  48.0          Sample atomic composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.0  0.55          Inner and outer radii (cm)
5          Sample height (cm)
3.211746011          Density Units:  gm/cm^3?
733.33          Temperature for sample Placzek correction
TRANSMISSION          Total cross section source
1.33812          Sample tweak factor
4.0          Top hat width (1/Å) for cleaning up Fourier Transform
0.3          Minimum radius for FT  [Å]
0.03          g(r) broadening at r = 1A [A]
0  0          0   0          to finish specifying wavelength range of resonance
0.0  1.0  0          Exponential amplitude and decay [1/A]
*  0  0          * 0 0 to specify end of exponential parameter input
1.0          Normalisation correction factor
*          Name of file containing self scattering as a function of wavelength [A]
0          Normalise to:Nothing
20.0          Maximum radius for FT [A]
0          Output units: b/atom/sr
0.0          Power for broadening function e.g. 0.5
0.01          Step size [A] 
0          Analyse this sample? 
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

CONTAINER 11mm Pt 827C          {

2  1          Number of  files and period number
SLS77043.raw          CONTAINER 11mm Pt 827C data files
SLS77044.raw          CONTAINER 11mm Pt 827C data files
Pt  0  1.0          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.537  0.55          Inner and outer radii (cm)
5          Sample height (cm)
20.94          Density Units:  gm/cm^3?
TRANSMISSION          Total cross section source
1.1          Tweak factor
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

GO          

SAMPLE BBS352 glass          {

10  1          Number of  files and period number
SLS77135.raw          SAMPLE BBS352 glass data files
SLS77136.raw          SAMPLE BBS352 glass data files
SLS77137.raw          SAMPLE BBS352 glass data files
SLS77138.raw          SAMPLE BBS352 glass data files
SLS77139.raw          SAMPLE BBS352 glass data files
SLS77140.raw          SAMPLE BBS352 glass data files
SLS77141.raw          SAMPLE BBS352 glass data files
SLS77142.raw          SAMPLE BBS352 glass data files
SLS77143.raw          SAMPLE BBS352 glass data files
SLS77144.raw          SAMPLE BBS352 glass data files
1          Force calculation of sample corrections?
B  11  95.904          Sample atomic composition
O  0  144.0          Sample atomic composition
B  10  0.096          Sample atomic composition
Ba  0  28.0          Sample atomic composition
O  0  28.0          Sample atomic composition
Si  0  24.0          Sample atomic composition
O  0  48.0          Sample atomic composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.0  0.55          Inner and outer radii (cm)
5          Sample height (cm)
3.138997055          Density Units:  gm/cm^3?
800          Temperature for sample Placzek correction
TRANSMISSION          Total cross section source
1.07917          Sample tweak factor
4.0          Top hat width (1/Å) for cleaning up Fourier Transform
0.3          Minimum radius for FT  [Å]
0.03          g(r) broadening at r = 1A [A]
0  0          0   0          to finish specifying wavelength range of resonance
0.0  1.0  0          Exponential amplitude and decay [1/A]
*  0  0          * 0 0 to specify end of exponential parameter input
1.0          Normalisation correction factor
*          Name of file containing self scattering as a function of wavelength [A]
0          Normalise to:Nothing
20.0          Maximum radius for FT [A]
0          Output units: b/atom/sr
0.0          Power for broadening function e.g. 0.5
0.01          Step size [A] 
1          Analyse this sample? 
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

CONTAINER 11mm Pt 927C          {

2  1          Number of  files and period number
SLS77046.raw          CONTAINER 11mm Pt 927C data files
SLS77047.raw          CONTAINER 11mm Pt 927C data files
Pt  0  1.0          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.537  0.55          Inner and outer radii (cm)
5          Sample height (cm)
20.87          Density Units:  gm/cm^3?
TRANSMISSION          Total cross section source
1.1          Tweak factor
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

GO          

SAMPLE BBS352 glass          {

8  1          Number of  files and period number
SLS77146.raw          SAMPLE BBS352 glass data files
SLS77147.raw          SAMPLE BBS352 glass data files
SLS77148.raw          SAMPLE BBS352 glass data files
SLS77149.raw          SAMPLE BBS352 glass data files
SLS77150.raw          SAMPLE BBS352 glass data files
SLS77151.raw          SAMPLE BBS352 glass data files
SLS77152.raw          SAMPLE BBS352 glass data files
SLS77153.raw          SAMPLE BBS352 glass data files
1          Force calculation of sample corrections?
B  11  95.904          Composition
O  0  144.0          Composition
B  10  0.096          Composition
Ba  0  28.0          Composition
O  0  28.0          Composition
Si  0  24.0          Composition
O  0  48.0          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.0  0.55          Inner and outer radii (cm)
5          Sample height (cm)
3.4529          Density Units:  gm/cm^3?
866.67          Temperature for Placzek correction:
TRANSMISSION          Total cross section source
2.353          Tweak factor
4.0          Top hat width (1/Å) for cleaning up Fourier Transform
0.3          Minimum radius for FT  [Å]
0.03          g(r) broadening at r = 1A [A]
0  0          0   0          to finish specifying wavelength range of resonance
0.0  1.0  0          Exponential amplitude and decay [1/A]
*  0  0          * 0 0 to specify end of exponential parameter input
1.0          Normalisation correction factor
*          Name of file containing self scattering as a function of wavelength [A]
0          Normalise to:Nothing
20.0          Maximum radius for FT [A]
0          Output units: b/atom/sr
0.0          Power for broadening function e.g. 0.5
0.01          Step size [A] 
0          Analyse this sample? 
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

CONTAINER 11mm Pt 1027C          {

2  1          Number of  files and period number
SLS77049.raw          CONTAINER 11mm Pt 1027C data files
SLS77050.raw          CONTAINER 11mm Pt 1027C data files
Pt  0  1.0          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.537  0.55          Inner and outer radii (cm)
5          Sample height (cm)
20.797          Density Units:  gm/cm^3?
TRANSMISSION          Total cross section source
1.1          Tweak factor
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

GO          

SAMPLE BBS352 glass          {

1  1          Number of  files and period number
SLS77145.raw          SAMPLE BBS352 glass data files
1          Force calculation of sample corrections?
B  11  95.904          Composition
O  0  144.0          Composition
B  10  0.096          Composition
Ba  0  28.0          Composition
O  0  28.0          Composition
Si  0  24.0          Composition
O  0  48.0          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.0  0.55          Inner and outer radii (cm)
5          Sample height (cm)
3.4529          Density Units:  gm/cm^3?
866.67          Temperature for Placzek correction:
TRANSMISSION          Total cross section source
2.353          Tweak factor
4.0          Top hat width (1/Å) for cleaning up Fourier Transform
0.3          Minimum radius for FT  [Å]
0.03          g(r) broadening at r = 1A [A]
0  0          0   0          to finish specifying wavelength range of resonance
0.0  1.0  0          Exponential amplitude and decay [1/A]
*  0  0          * 0 0 to specify end of exponential parameter input
1.0          Normalisation correction factor
*          Name of file containing self scattering as a function of wavelength [A]
0          Normalise to:Nothing
20.0          Maximum radius for FT [A]
0          Output units: b/atom/sr
0.0          Power for broadening function e.g. 0.5
0.01          Step size [A] 
0          Analyse this sample? 
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

CONTAINER 11mm Pt 1027C          {

2  1          Number of  files and period number
SLS77049.raw          CONTAINER 11mm Pt 1027C data files
SLS77050.raw          CONTAINER 11mm Pt 1027C data files
Pt  0  1.0          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.537  0.55          Inner and outer radii (cm)
5          Sample height (cm)
20.797          Density Units:  gm/cm^3?
TRANSMISSION          Total cross section source
0.9          Tweak factor
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

GO          

SAMPLE BBS352 glass          {

1  1          Number of  files and period number
SLS77154.raw          SAMPLE BBS352 glass data files
1          Force calculation of sample corrections?
B  11  95.904          Composition
O  0  144.0          Composition
B  10  0.096          Composition
Ba  0  28.0          Composition
O  0  28.0          Composition
Si  0  24.0          Composition
O  0  48.0          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.0  0.55          Inner and outer radii (cm)
5          Sample height (cm)
3.4529          Density Units:  gm/cm^3?
933.33          Temperature for Placzek correction:
TRANSMISSION          Total cross section source
2.353          Tweak factor
4.0          Top hat width (1/Å) for cleaning up Fourier Transform
0.3          Minimum radius for FT  [Å]
0.03          g(r) broadening at r = 1A [A]
0  0          0   0          to finish specifying wavelength range of resonance
0.0  1.0  0          Exponential amplitude and decay [1/A]
*  0  0          * 0 0 to specify end of exponential parameter input
1.0          Normalisation correction factor
*          Name of file containing self scattering as a function of wavelength [A]
0          Normalise to:Nothing
20.0          Maximum radius for FT [A]
0          Output units: b/atom/sr
0.0          Power for broadening function e.g. 0.5
0.01          Step size [A] 
0          Analyse this sample? 
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

CONTAINER 11mm Pt 1127C          {

2  1          Number of  files and period number
SLS77052.raw          CONTAINER 11mm Pt 1127C data files
SLS77054.raw          CONTAINER 11mm Pt 1127C data files
Pt  0  1.0          Composition
*  0  0          * 0 0 to specify end of composition input
SameAsBeam          Geometry
0.537  0.55          Inner and outer radii (cm)
5          Sample height (cm)
20.72          Density Units:  gm/cm^3?
TRANSMISSION          Total cross section source
1.1          Tweak factor
1.0  0.0          Sample environment scattering fraction and attenuation coefficient [per A]

}

GO          


END          
1 2 3 4 5 6 7 8 9 10
Date and time last written:  20250226 13:57:26          
N